\subsection{Step- and Turn-Detection}
	
	used for the transition step
	uses the smartphone's imu (acc, gyro)
	simple step detection using magnitudes
	simple turn detection by integrating over the gyro
	feeds the transition 
